; version 9 - module specs, also see s303.txt for text substitutions.
0 Invalid
remarks "not an actual module type"
cycles 0.00000
progMem 0.00000
xmem 0.00000
ymem 0.00000
zeropage 0.00000
dynmem 0.00000
height 0
parameters
inputs
outputs
custom
----------
1 Keyboard
remarks "only 1"
cycles 0.00000
progMem 0.00000
xmem 0.00000
ymem 0.00000
zeropage 3.00000
dynmem 1.00000
height 2
parameters
inputs
outputs
0 "Note" control
1 "gate" logic
2 "velocity on" control
3 "velocity off" control
custom
----------
2 AudioIn
remarks ""
cycles 2.20000
progMem 1.00000
xmem 1.00000
ymem 1.00000
zeropage 2.00000
dynmem 1.00000
height 2
parameters
inputs
outputs
0 "left" audio
1 "right" audio
custom
----------
3 4Output
remarks ""
cycles 2.06250
progMem 0.46875
xmem 0.09375
ymem 0.00000
zeropage 0.00000
dynmem 0.28125
height 3
parameters
0 "level" 0..127 ""
inputs
0 "out 1" audio
1 "out 2" audio
2 "out 3" audio
3 "out 4" audio
outputs
custom
----------
4 2Output
remarks ""
cycles 1.40625
progMem 0.34375
xmem 0.09375
ymem 0.09375
zeropage 0.00000
dynmem 0.37500
height 3
parameters
0 "level" 0..127 ""
1 "destination" 0..2 "2destination"
2 "mute" 0..1 "onoff"
inputs
0 "out left" audio
1 "out right" audio
outputs
custom
----------
5 1Output
remarks ""
cycles 1.28125
progMem 0.31250
xmem 0.09375
ymem 0.09375
zeropage 0.00000
dynmem 0.37500
height 3
parameters
0 "level" 0..127 ""
1 "destination" 0..5 "1destination"
2 "mute" 0..1 "onoff"
inputs
0 "out" audio
outputs
custom
----------
7 OscA
remarks ""
cycles 10.81250
progMem 6.56250
xmem 0.84375
ymem 0.34375
zeropage 1.75000
dynmem 0.37500
height 6
parameters
0 "freq coarse" 0..127 "freqcoarse"
1 "freq fine" 0..127 "freqfine"
2 "kbt" 0..127 "freqkbt"
3 "Pulse width" 0..127 "pulsewidth"
4 "waveform" 0..3 "waveform1"
5 "pitch mod 1" 0..127 ""
6 "pitch mod 2" 0..127 ""
7 "fm mod" 0..127 ""
8 "PW mod" 0..127 ""
9 "Mute" 0..1 "onoff"
inputs
0 "sync" audio
1 "fm mod" audio
2 "pitch mod 1" audio
3 "pitch mod 2" audio
4 "pw mod" audio
outputs
0 "out" audio
1 "slv" slave
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
8 OscB
remarks ""
cycles 8.28125
progMem 6.25000
xmem 0.68750
ymem 0.50000
zeropage 1.75000
dynmem 0.68750
height 6
parameters
0 "Freq coarse" 0..127 "freqcoarse"
1 "Freq fine" 0..127 "freqfine"
2 "kbt" 0..127 "freqkbt"
3 "waveform" 0..3 "waveform1"
4 "pitch mod 1" 0..127 ""
5 "pitch mod 2" 0..127 ""
6 "fm mod" 0..127 ""
7 "pw mod" 0..127 "pulsewidth"
8 "mute" 0..1 "onoff"
inputs
0 "fm mod" audio
1 "pitch mod 1" control
2 "pitch mod 2" control
3 "pw mod" control
outputs
0 "out" audio
1 "slv" slave
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
9 OscC
remarks ""
cycles 4.96875
progMem 1.09375
xmem 0.56250
ymem 0.09375
zeropage 1.75000
dynmem 0.53125
height 4
parameters
0 "freq coarse" 0..127 "freqcoarse"
1 "freq fine" 0..127 "freqfine"
2 "kbt" 0..1 "onoff"
3 "freq mod" 0..127 ""
4 "fm mod" 0..127 ""
5 "mute" 0..1 "onoff"
inputs
0 "fm mod" audio
1 "pitch" audio
2 "AM" audio
outputs
0 "out" audio
1 "slv" slave
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
10 OscSlvB
remarks ""
cycles 7.12500
progMem 2.15625
xmem 0.21875
ymem 0.34375
zeropage 0.87500
dynmem 0.50000
height 3
parameters
0 "detune coarse" 0..127 "symetric"
1 "detune fine" 0..127 "symetric"
2 "Pulse Width" 0..127 "pulsewidth"
3 "pw mod" 0..127 ""
4 "mute" 0..1 "onoff"
inputs
0 "mst" slave
1 "pw mod" audio
outputs
0 "out" audio
custom
0 "freq display units" 0..2 "freqdisplunits3"
----------
11 OscSlvC
remarks ""
cycles 6.00000
progMem 1.75000
xmem 0.15625
ymem 0.21875
zeropage 0.87500
dynmem 0.50000
height 3
parameters
0 "detune coarse" 0..127 "symetric"
1 "detune fine" 0..127 "symetric"
2 "fm mod" 0..127 ""
3 "mute" 0..1 "onoff"
inputs
0 "mst" slave
1 "fm mod" audio
outputs
0 "out" audio
custom
0 "freq display units" 0..2 "freqdisplunits3"
----------
12 OscSlvD
remarks ""
cycles 5.87500
progMem 1.31250
xmem 0.15625
ymem 0.21875
zeropage 0.87500
dynmem 0.43750
height 3
parameters
0 "detune coarse" 0..127 "symetric"
1 "detune fine" 0..127 "symetric"
2 "fm mod" 0..127 ""
3 "mute" 0..1 "onoff"
inputs
0 "mst" slave
1 "fm mod" audio
outputs
0 "out" audio
custom
0 "freq display units" 0..2 "freqdisplunits3"
----------
13 OscSlvE
remarks ""
cycles 3.06250
progMem 0.68750
xmem 0.34375
ymem 0.15625
zeropage 0.87500
dynmem 0.43750
height 3
parameters
0 "detune coarse" 0..127 "symetric"
1 "detune fine" 0..127 "symetric"
2 "fm mod" 0..127 ""
3 "mute" 0..1 "onoff"
inputs
0 "mst" slave
1 "fm mod" audio
2 "AM" audio
outputs
0 "out" audio
custom
0 "freq display units" 0..2 "freqdisplunits3"
----------
14 OscSlvA
remarks ""
cycles 7.62500
progMem 5.87500
xmem 0.43750
ymem 0.28125
zeropage 0.87500
dynmem 0.50000
height 4
parameters
0 "detune coarse" 0..127 "symetric"
1 "detune fine" 0..127 "symetric"
2 "waveform" 0..3 ""
3 "fm mod" 0..127 ""
4 "mute" 0..1 "onoff"
inputs
0 "mst" slave
1 "fm mod" audio
2 "AM" audio
3 "sync" audio
outputs
0 "out" audio
custom
0 "freq display units" 0..2 "freqdisplunits3"
----------
15 NoteSeqA
remarks ""
cycles 1.43750
progMem 1.15625
xmem 0.56250
ymem 1.43750
zeropage 3.50000
dynmem 1.25000
height 7
parameters
0 "note 1" 0..127 "symetric"
1 "note 2" 0..127 "symetric"
2 "note 3" 0..127 "symetric"
3 "note 4" 0..127 "symetric"
4 "note 5" 0..127 "symetric"
5 "note 6" 0..127 "symetric"
6 "note 7" 0..127 "symetric"
7 "note 8" 0..127 "symetric"
8 "note 9" 0..127 "symetric"
9 "note 10" 0..127 "symetric"
10 "note 11" 0..127 "symetric"
11 "note 12" 0..127 "symetric"
12 "note 13" 0..127 "symetric"
13 "note 14" 0..127 "symetric"
14 "note 15" 0..127 "symetric"
15 "note 16" 0..127 "symetric"
16 "length" 0..15 ""
17 "edit position" 0..16 "editpos"
18 "record" 0..1 "onoff"
19 "pause" 0..1 "onoff"
20 "loop" 0..1 "onoff"
inputs
0 "clk" logic
1 "reset" logic
outputs
0 "out" control
1 "snc" logic
2 "link" logic
3 "gclk" logic
custom
----------
16 PortamentoB
remarks ""
cycles 0.53125
progMem 0.46875
xmem 0.15625
ymem 0.21875
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "time" 0..127 "adsrtime"
inputs
0 "in" control
1 "jmp" logic
outputs
0 "out" control
custom
----------
17 EventSeq
remarks ""
cycles 1.65625
progMem 1.34375
xmem 0.62500
ymem 1.43750
zeropage 3.50000
dynmem 2.00000
height 5
parameters
0 "length" 0..15 ""
1 "loop" 0..1 "onoff"
2 "gate1" 0..1 "onoff"
3 "gate2" 0..1 "onoff"
4 "seq 1 step 1" 0..1 "onoff"
5 "seq 1 step 2" 0..1 "onoff"
6 "seq 1 step 3" 0..1 "onoff"
7 "seq 1 step 4" 0..1 "onoff"
8 "seq 1 step 5" 0..1 "onoff"
9 "seq 1 step 6" 0..1 "onoff"
10 "seq 1 step 7" 0..1 "onoff"
11 "seq 1 step 8" 0..1 "onoff"
12 "seq 1 step 9" 0..1 "onoff"
13 "seq 1 step 10" 0..1 "onoff"
14 "seq 1 step 11" 0..1 "onoff"
15 "seq 1 step 12" 0..1 "onoff"
16 "seq 1 step 13" 0..1 "onoff"
17 "seq 1 step 14" 0..1 "onoff"
18 "seq 1 step 15" 0..1 "onoff"
19 "seq 1 step 16" 0..1 "onoff"
20 "seq 2 step 1" 0..1 "onoff"
21 "seq 2 step 2" 0..1 "onoff"
22 "seq 2 step 3" 0..1 "onoff"
23 "seq 2 step 4" 0..1 "onoff"
24 "seq 2 step 5" 0..1 "onoff"
25 "seq 2 step 6" 0..1 "onoff"
26 "seq 2 step 7" 0..1 "onoff"
27 "seq 2 step 8" 0..1 "onoff"
28 "seq 2 step 9" 0..1 "onoff"
29 "seq 2 step 10" 0..1 "onoff"
30 "seq 2 step 11" 0..1 "onoff"
31 "seq 2 step 12" 0..1 "onoff"
32 "seq 2 step 13" 0..1 "onoff"
33 "seq 2 step 14" 0..1 "onoff"
34 "seq 2 step 15" 0..1 "onoff"
35 "seq 2 step 16" 0..1 "onoff"
inputs
0 "clk" logic
1 "rst" logic
outputs
0 "out1" logic
1 "out2" logic
2 "snc" logic
3 "link" logic
custom
----------
18 X-Fade
remarks ""
cycles 1.65625
progMem 0.40625
xmem 0.09375
ymem 0.15625
zeropage 0.87500
dynmem 0.34375
height 3
parameters
0 "mix mod" 0..127 ""
1 "mix" 0..127 "symetric"
inputs
0 "in1" audio
1 "in2" audio
2 "mix mod" audio
outputs
0 "out" audio
custom
----------
19 3Mixer
remarks "3 input mixer"
cycles 0.90625
progMem 0.21875
xmem 0.15625
ymem 0.09375
zeropage 0.87500
dynmem 0.37500
height 2
parameters
0 "lev 1" 0..127 ""
1 "lev 2" 0..127 ""
2 "lev 3" 0..127 ""
inputs
0 "in1" audio
1 "in2" audio
2 "in3" audio
outputs
0 "out" audio
custom
----------
20 ADSR-Env
remarks ""
cycles 1.62500
progMem 1.06250
xmem 1.03125
ymem 0.21875
zeropage 1.75000
dynmem 0.53125
height 5
parameters
0 "attack shape" 0..2 "adsrshape"
1 "attack" 0..127 "adsrtime"
2 "decay" 0..127 "adsrtime"
3 "sustain" 0..127 ""
4 "release" 0..127 "adsrtime"
5 "invert" 0..1 "onoff"
inputs
0 "in" audio
1 "gate" logic
2 "retrig" logic
3 "amp" control
outputs
0 "env" control
1 "out" audio
custom
----------
21 Compressor
remarks ""
cycles 8.28125
progMem 1.81250
xmem 0.56250
ymem 0.56250
zeropage 1.75000
dynmem 0.68750
height 7
parameters
0 "attack" 0..127 "companderattack"
1 "release" 0..127 "companderrelease"
2 "threshold" 0..42 "compandertreshold"
3 "ratio" 0..66 "companderratio"
4 "ref level" 0..42 "companderref"
5 "limiter" 0..24 "companderlimit"
6 "act" 0..1 "onoff"
7 "mon" 0..1 "onoff"
8 "bypass" 0..1 "onoff"
inputs
0 "left" audio
1 "right" audio
2 "side" audio
outputs
0 "left" audio
1 "right" audio
custom
----------
22 PartialGen
remarks ""
cycles 0.59375
progMem 0.53125
xmem 0.28125
ymem 2.18750
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "range" 0..127 "symetric"
inputs
0 "in" control
outputs
0 "out" control
custom
----------
23 Mod-Env
remarks ""
cycles 3.34375
progMem 2.53125
xmem 2.59375
ymem 0.15625
zeropage 1.75000
dynmem 0.68750
height 6
parameters
0 "attack" 0..127 "adsrtime"
1 "decay" 0..127 "adsrtime"
2 "sustain" 0..127 ""
3 "release" 0..127 "adsrtime"
4 "attack mod" 0..127 ""
5 "decay mod" 0..127 ""
6 "sustain mod" 0..127 ""
7 "release mod" 0..127 ""
8 "invert" 0..1 "onoff"
inputs
0 "gate" logic
1 "retrig" logic
2 "attack mod" control
3 "decay mod" control
4 "sustain mod" control
5 "release mod" control
6 "in" audio
7 "amp" control
outputs
0 "env" control
1 "out" audio
custom
----------
24 LFOA
remarks ""
cycles 1.78125
progMem 2.37500
xmem 0.56250
ymem 0.21875
zeropage 1.75000
dynmem 0.62500
height 5
parameters
0 "rate" 0..127 "lforate"
1 "range" 0..2 "lforange"
2 "waveform" 0..4 "lfoshape"
3 "rate mod" 0..127 ""
4 "mono" 0..1 "onoff"
5 "kbt" 0..127 "freqkbt"
6 "phase" 0..127 "phase"
7 "mute" 0..1 "onoff"
inputs
0 "rate" control
1 "reset" logic
outputs
0 "slv" slave
1 "out" control
custom
----------
25 LFOB
remarks ""
cycles 1.18750
progMem 1.06250
xmem 0.50000
ymem 0.28125
zeropage 1.75000
dynmem 0.62500
height 5
parameters
0 "rate" 0..127 "lforate"
1 "range" 0..2 "lforange"
2 "phase" 0..127 "phase"
3 "rate mod" 0..127 ""
4 "mono" 0..1 "onoff"
5 "kbt" 0..127 "freqkbt"
6 "PW mod" 0..127 ""
7 "PW" 0..127 "pulsewidth"
inputs
0 "rate" control
1 "rst" logic
2 "PWmod" control
outputs
0 "out" control
1 "slv" slave
custom
----------
26 LFOC
remarks ""
cycles 1.46875
progMem 1.06250
xmem 0.50000
ymem 0.15625
zeropage 1.75000
dynmem 0.50000
height 4
parameters
0 "rate" 0..127 "lforate"
1 "range" 0..2 "lforange"
2 "waveform" 0..4 "lfoshape"
3 "rate mod" 0..127 ""
4 "mono" 0..1 "onoff"
5 "mute" 0..1 "onoff"
inputs
0 "rate" control
outputs
0 "out" control
1 "slv" slave
custom
----------
27 LFOSlvB
remarks ""
cycles 0.37500
progMem 0.34375
xmem 0.09375
ymem 0.15625
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "rate" 0..127 "lfoslvrate"
inputs
0 "mst" slave
outputs
0 "out" control
custom
0 "freq display units" 0..1 "freqdisplunitslfo"
----------
28 LFOSlvC
remarks ""
cycles 0.78125
progMem 0.68750
xmem 0.34375
ymem 0.15625
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "rate" 0..127 "lfoslvrate"
inputs
0 "mst" slave
outputs
0 "out" control
custom
0 "freq display units" 0..1 "freqdisplunitslfo"
----------
29 LFOSlvD
remarks ""
cycles 0.37500
progMem 0.34375
xmem 0.15625
ymem 0.15625
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "rate" 0..127 "lfoslvrate"
inputs
0 "mst" slave
outputs
0 "out" control
custom
0 "freq display units" 0..1 "freqdisplunitslfo"
----------
30 LFOSlvE
remarks ""
cycles 0.34375
progMem 0.31250
xmem 0.15625
ymem 0.15625
zeropage 0.90625
dynmem 0.28125
height 2
parameters
0 "rate" 0..127 "lfoslvrate"
inputs
0 "mst" slave
outputs
0 "out" control
custom
0 "freq display units" 0..1 "freqdisplunitslfo"
----------
31 Noise
remarks ""
cycles 1.65625
progMem 0.40625
xmem 0.28125
ymem 0.15625
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "color" 0..127 "noisecolor"
inputs
outputs
0 "out" audio
custom
----------
32 FilterBank
remarks ""
cycles 17.93750
progMem 9.00000
xmem 5.59375
ymem 10.21875
zeropage 0.90625
dynmem 0.96875
height 7
parameters
0 "50" 0..127 ""
1 "75" 0..127 ""
2 "110" 0..127 ""
3 "170" 0..127 ""
4 "250" 0..127 ""
5 "380" 0..127 ""
6 "570" 0..127 ""
7 "850" 0..127 ""
8 "1.3" 0..127 ""
9 "1.9" 0..127 ""
10 "2.9" 0..127 ""
11 "4.2" 0..127 ""
12 "6.4" 0..127 ""
13 "8.3" 0..127 ""
14 "bypass" 0..1 ""
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
33 ClkRndGen
remarks ""
cycles 0.62500
progMem 0.62500
xmem 0.21875
ymem 0.21875
zeropage 0.87500
dynmem 0.34375
height 2
parameters
0 "mono" 0..1 "onoff"
1 "color" 0..1 "onoff"
inputs
0 "clk" logic
outputs
0 "out" control
custom
----------
34 RndStepGen
remarks ""
cycles 0.62500
progMem 0.65625
xmem 0.21875
ymem 0.34375
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "rate" 0..127 "lfoslvrate"
inputs
0 "mst" slave
outputs
0 "out" control
custom
----------
35 RndPulsGen
remarks ""
cycles 0.34375
progMem 0.31250
xmem 0.21875
ymem 0.15625
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "density" 0..127 ""
inputs
outputs
0 "out" logic
custom
----------
36 PosEdgeDelay
remarks ""
cycles 0.28125
progMem 0.25000
xmem 0.15625
ymem 0.15625
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "time" 0..127 "logictime"
inputs
0 "in" logic
outputs
0 "out" logic
custom
----------
37 LogicDelay
remarks ""
cycles 0.62500
progMem 0.56250
xmem 0.15625
ymem 0.28125
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "time" 0..127 "logictime"
inputs
0 "in" logic
outputs
0 "out" logic
custom
----------
38 Pulse
remarks ""
cycles 0.34375
progMem 0.31250
xmem 0.21875
ymem 0.15625
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "time" 0..127 "logictime"
inputs
0 "in" logic
outputs
0 "out" logic
custom
----------
39 Smooth
remarks ""
cycles 0.25000
progMem 0.21875
xmem 0.09375
ymem 0.09375
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "time" 0..127 "smoothtime"
inputs
0 "in" control
outputs
0 "out" control
custom
----------
40 8Mixer
remarks "8 input mixer"
cycles 2.18750
progMem 0.50000
xmem 0.28125
ymem 0.34375
zeropage 0.90625
dynmem 0.68750
height 4
parameters
0 "lev 1" 0..127 ""
1 "lev 2" 0..127 ""
2 "lev 3" 0..127 ""
3 "lev 4" 0..127 ""
4 "lev 5" 0..127 ""
5 "lev 6" 0..127 ""
6 "lev 7" 0..127 ""
7 "lev 8" 0..127 ""
8 "-6dB" 0..1 ""
inputs
0 "in 1" audio
1 "in 2" audio
2 "in 3" audio
3 "in 4" audio
4 "in 5" audio
5 "in 6" audio
6 "in 7" audio
7 "in 8" audio
outputs
0 "out" audio
custom
----------
43 Constant
remarks ""
cycles 0.00000
progMem 0.00000
xmem 0.00000
ymem 0.00000
zeropage 0.87500
dynmem 0.34375
height 2
parameters
0 "value" 0..127 "unibi"
1 "unipolar" 0..1 "onoff"
inputs
outputs
0 "out" control
custom
----------
44 GainControl
remarks ""
cycles 0.78125
progMem 0.21875
xmem 0.09375
ymem 0.00000
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "shift" 0..1 "onoff"
inputs
0 "control" audio
1 "in" audio
outputs
0 "out" audio
custom
----------
45 VocalFilter
remarks ""
cycles 7.59375
progMem 3.06250
xmem 1.78125
ymem 2.06250
zeropage 0.87500
dynmem 0.68750
height 5
parameters
0 "vowel1" 0..8 "vowel"
1 "vowel2" 0..8 "vowel"
2 "vowel3" 0..8 "vowel"
3 "level" 0..127 ""
4 "vowel" 0..127 "symeteric"
5 "vowel mod" 0..127 ""
6 "freq" 0..127 "symetric"
7 "freq mod" 0..127 ""
8 "res" 0..127 ""
inputs
0 "in" audio
1 "vowel mod" control
2 "frequency mod" control
outputs
0 "out" audio
custom
----------
46 AHD-Env
remarks ""
cycles 2.46875
progMem 1.75000
xmem 1.31250
ymem 0.21875
zeropage 1.75000
dynmem 0.53125
height 5
parameters
0 "Attack" 0..127 "adsrtime"
1 "Hold" 0..127 "adsrtime"
2 "Decay" 0..127 "adsrtime"
3 "Attack mod" 0..127 ""
4 "Hold mod" 0..127 ""
5 "Decay mod" 0..127 ""
inputs
0 "trig" logic
1 "Attack mod" control
2 "Hold mod" control
3 "Decay mod" control
4 "in" audio
5 "amp" control
outputs
0 "env" control
1 "out" audio
custom
----------
47 Pan
remarks ""
cycles 1.65625
progMem 0.40625
xmem 0.09375
ymem 0.09375
zeropage 1.75000
dynmem 0.34375
height 3
parameters
0 "pan mod" 0..127 ""
1 "pan" 0..127 "symetric"
inputs
0 "in" audio
1 "panmod" audio
outputs
0 "outL" audio
1 "outR" audio
custom
----------
48 PortamentoA
remarks ""
cycles 0.46875
progMem 0.43750
xmem 0.09375
ymem 0.21875
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "time" 0..127 "adsrtime"
inputs
0 "in" control
1 "on" logic
outputs
0 "out" control
custom
----------
49 FilterD
remarks ""
cycles 4.03125
progMem 1.53125
xmem 0.56250
ymem 0.43750
zeropage 2.62500
dynmem 0.43750
height 5
parameters
0 "freq" 0..127 "filterfreq"
1 "kbt" 0..127 "freqkbt"
2 "res" 0..127 ""
3 "freq mod" 0..127 ""
inputs
0 "freq mod" control
1 "in" audio
outputs
0 "hp" audio
1 "bp" audio
2 "lp" audio
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
50 FilterC
remarks ""
cycles 1.78125
progMem 0.43750
xmem 0.21875
ymem 0.15625
zeropage 2.62500
dynmem 0.40625
height 4
parameters
0 "freq" 0..127 "filterfreq"
1 "res" 0..127 ""
2 "gain control" 0..1 "onoff"
inputs
0 "in" audio
outputs
0 "LP" audio
1 "BP" audio
2 "HP" audio
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
51 FilterE
remarks ""
cycles 6.62500
progMem 1.46875
xmem 0.56250
ymem 0.62500
zeropage 0.87500
dynmem 0.75000
height 6
parameters
0 "filter type" 0..3 "filtertype"
1 "gain control" 0..1 "onoff"
2 "freq mod 1" 0..127 ""
3 "freq" 0..127 "filterfreq"
4 "kbt" 0..127 "freqkbt"
5 "res mod" 0..127 ""
6 "res" 0..127 ""
7 "slope" 0..1 "filterslope2"
8 "freq mod 2" 0..127 ""
9 "bypass" 0..1 "onoff"
inputs
0 "freq mod 1" audio
1 "res mod" audio
2 "in" audio
3 "freq mod 2" audio
outputs
0 "out" audio
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
52 Multi-Env
remarks ""
cycles 1.96875
progMem 1.40625
xmem 2.53125
ymem 0.43750
zeropage 1.75000
dynmem 0.78125
height 7
parameters
0 "level 1" 0..127 ""
1 "level 2" 0..127 ""
2 "level 3" 0..127 ""
3 "level 4" 0..127 ""
4 "time 1" 0..127 "adsrtime"
5 "time 2" 0..127 "adsrtime"
6 "time 3" 0..127 "adsrtime"
7 "time 4" 0..127 "adsrtime"
8 "time 5" 0..127 "adsrtime"
9 "sustain" 0..4 "0 ~ off, 4 ~ level 4"
10 "curve" 0..2 "0 ~ bipolar, 1 ~ uni/exp, 2 ~ uni/lin"
inputs
0 "gate" logic
1 "in" audio
2 "amp" control
outputs
0 "env" control
1 "out" audio
custom
----------
53 Sample&Hold
remarks ""
cycles 1.03125
progMem 0.25000
xmem 0.00000
ymem 0.09375
zeropage 0.87500
dynmem 0.25000
height 2
parameters
inputs
0 "trig" logic
1 "in" audio
outputs
0 "out" audio
custom
----------
54 Quantizer
remarks ""
cycles 0.53125
progMem 0.15625
xmem 0.09375
ymem 0.00000
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "bits" 0..12 "quantbits"
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
57 InvLevShift
remarks ""
cycles 0.53125
progMem 0.15625
xmem 0.09375
ymem 0.09375
zeropage 0.87500
dynmem 0.34375
height 2
parameters
0 "mode" 0..2 "0 ~ bipolar, 1 ~ uni/neg, 2 ~ uni/pos"
1 "inv" 0..1 "onoff"
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
58 DrumSynth
remarks "preset info is not saved into the patch"
cycles 12.21875
progMem 4.71875
xmem 2.18750
ymem 1.81250
zeropage 0.87500
dynmem 1.03125
height 9
parameters
0 "masterfreq" 0..127 ""
1 "slave ratio" 0..127 ""
2 "master decay" 0..127 ""
3 "slave decay" 0..127 ""
4 "master level" 0..127 ""
5 "slave level" 0..127 ""
6 "noise flt freq" 0..127 ""
7 "noise flt res" 0..127 ""
8 "noise flt sweep" 0..127 ""
9 "noise flt decay" 0..127 ""
10 "noise flt mode" 0..2 "filtertype1"
11 "bend amount" 0..127 ""
12 "bend decay" 0..127 ""
13 "click" 0..127 ""
14 "noise" 0..127 ""
15 "Mute" 0..1 "onoff"
inputs
0 "trig" logic
1 "vel" control
2 "pitch" control
outputs
0 "out" audio
custom
----------
59 CompareLev
remarks ""
cycles 0.18750
progMem 0.18750
xmem 0.09375
ymem 0.09375
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "level" 0..127 "symetric"
inputs
0 "in" control
outputs
0 "out" logic
custom
----------
61 Clip
remarks ""
cycles 1.53125
progMem 0.37500
xmem 0.09375
ymem 0.15625
zeropage 0.87500
dynmem 0.37500
height 3
parameters
0 "clip mod" 0..127 ""
1 "clip" 0..127 ""
2 "sym" 0..1 ""
inputs
0 "in" audio
1 "clip" audio
outputs
0 "out" audio
custom
----------
62 Overdrive
remarks ""
cycles 4.00000
progMem 1.65625
xmem 0.28125
ymem 0.34375
zeropage 0.87500
dynmem 0.34375
height 3
parameters
0 "overdrive mod" 0..127 ""
1 "overdrive" 0..127 ""
inputs
0 "in" audio
1 "overdrive mod" control
outputs
0 "out" audio
custom
----------
63 KeyboardPatch
remarks "only 1"
cycles 0.00000
progMem 0.00000
xmem 0.00000
ymem 0.00000
zeropage 4.00000
dynmem 1.00000
height 3
parameters
inputs
outputs
0 "latest note" control
1 "patch gate" logic
2 "latest vel on" control
3 "latest rel vel" control
custom
----------
64 NegEdgeDelay
remarks ""
cycles 0.28125
progMem 0.25000
xmem 0.15625
ymem 0.15625
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "time" 0..127 "logictime"
inputs
0 "in" logic
outputs
0 "out" logic
custom
----------
65 MIDIGlobal
remarks "only 1"
cycles 0.13000
progMem 1.00000
xmem 1.00000
ymem 0.00000
zeropage 1.00000
dynmem 1.00000
height 2
parameters
inputs
outputs
0 "clk" logic
1 "sync" logic
2 "active" logic
custom
----------
66 ControlMixer
remarks ""
cycles 0.18750
progMem 0.18750
xmem 0.09375
ymem 0.09375
zeropage 0.87500
dynmem 0.46875
height 2
parameters
0 "inv 1" 0..1 "onoff"
1 "level 1" 0..127 ""
2 "inv 2" 0..1 "onoff"
3 "level 2" 0..127 ""
4 "mode" 0..1 "0 ~ lin, 1 ~ exp"
inputs
0 "in1" control
1 "in2" control
outputs
0 "out" control
custom
----------
67 NoteDetect
remarks ""
cycles 0.00000
progMem 0.00000
xmem 0.00000
ymem 0.00000
zeropage 2.65625
dynmem 0.28125
height 2
parameters
0 "note" 0..127 "freqcoarse"
inputs
outputs
0 "gate" logic
1 "velocity" control
2 "releasevelocity" control
custom
----------
68 ClkGen
remarks ""
cycles 1.00000
progMem 0.78125
xmem 0.43750
ymem 0.28125
zeropage 3.53125
dynmem 0.34375
height 3
parameters
0 "rate" 0..127 ""
1 "on/off" 0..1 "onoff"
inputs
0 "rst" logic
outputs
0 "24 pulses / beat" logic
1 "4 pulses / beat" logic
2 "slv" slave
3 "sync" logic
custom
----------
69 ClkDiv
remarks ""
cycles 0.62500
progMem 0.56250
xmem 0.50000
ymem 0.09375
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "divider" 0..127 "logicdiv"
inputs
0 "clk" logic
1 "rst" logic
outputs
0 "out" logic
custom
----------
70 LogicInv
remarks ""
cycles 0.18750
progMem 0.18750
xmem 0.09375
ymem 0.00000
zeropage 0.87500
dynmem 0.25000
height 2
parameters
inputs
0 "in" logic
outputs
0 "out" logic
custom
----------
71 EnvFollower
remarks ""
cycles 2.31250
progMem 0.50000
xmem 0.21875
ymem 0.15625
zeropage 0.87500
dynmem 0.34375
height 3
parameters
0 "attack" 0..127 ""
1 "release" 0..127 ""
inputs
0 "in" audio
outputs
0 "out" control
custom
----------
72 NoteScaler
remarks ""
cycles 0.15625
progMem 0.15625
xmem 0.09375
ymem 0.09375
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "transpose" 0..127 ""
inputs
0 "in" control
outputs
0 "out" control
custom
----------
73 LogicProc
remarks ""
cycles 0.28125
progMem 0.25000
xmem 0.09375
ymem 0.00000
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "mode" 0..2 "0 ~ and, 1 ~ or, 2 ~ xor"
inputs
0 "in1" logic
1 "in2" logic
outputs
0 "out" logic
custom
----------
74 WaveWrap
remarks ""
cycles 2.68750
progMem 0.62500
xmem 0.09375
ymem 0.15625
zeropage 0.87500
dynmem 0.34275
height 3
parameters
0 "wrap mod" 0..127 ""
1 "wrap" 0..127 ""
inputs
0 "in" audio
1 "wrap mod" audio
outputs
0 "out" audio
custom
----------
75 NoteQuant
remarks ""
cycles 0.43750
progMem 0.40625
xmem 0.15625
ymem 0.09375
zeropage 0.87500
dynmem 0.34375
height 2
parameters
0 "range" 0..127 "symetric"
1 "notes" 0..127 "0 ~ off"
inputs
0 "in" control
outputs
0 "out" control
custom
----------
76 OnOff
remarks ""
cycles 0.40625
progMem 0.12500
xmem 0.00000
ymem 0.00000
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "on" 0..1 ""
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
77 ClkDivFix
remarks ""
cycles 0.84375
progMem 0.75000
xmem 0.43750
ymem 0.09375
zeropage 2.62500
dynmem 0.25000
height 2
parameters
inputs
0 "reset" logic
1 "midi clock" logic
outputs
0 "16" logic
1 "T8" logic
2 "8" logic
custom
----------
78 Delay
remarks "audio delay"
cycles 8.00000
progMem 1.84375
xmem 9.25000
ymem 9.25000
zeropage 1.75000
dynmem 0.34375
height 3
parameters
0 "modulation" 0..127 ""
1 "time" 0..127 "0 ~ 0 ms, 127 ~ 2.65 ms"
inputs
0 "in" audio
1 "modulation" control
outputs
0 "2.65 ms fixed delay" audio
1 "variable delay out" audio
custom
----------
79 4-1Switch
remarks ""
cycles 1.03125
progMem 0.21875
xmem 0.28125
ymem 0.15625
zeropage 0.87500
dynmem 0.53125
height 3
parameters
0 "sel" 0..3 ""
1 "level 1" 0..127 ""
2 "level 2" 0..127 ""
3 "level 3" 0..127 ""
4 "level 4" 0..127 ""
5 "mute" 0..1 "onoff"
inputs
0 "in 1" audio
1 "in 2" audio
2 "in 3" audio
3 "in 4" audio
outputs
0 "out" audio
custom
----------
80 LFOSlvA
remarks ""
cycles 1.21875
progMem 1.90625
xmem 0.43750
ymem 0.21875
zeropage 0.87500
dynmem 0.50000
height 4
parameters
0 "rate" 0..127 "lfoslvrate"
1 "phase" 0..127 "phase"
2 "waveform" 0..4 "lfoshape"
3 "mono" 0..1 "onoff"
4 "mute" 0..1 "onoff"
inputs
0 "mst" slave
1 "reset" logic
outputs
0 "out" control
custom
0 "freq display units" 0..1 "freqdisplunitslfo"
----------
81 Amplifier
remarks ""
cycles 0.65625
progMem 0.18750
xmem 0.09375
ymem 0.00000
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "gain" 0..127 "ampgain"
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
82 Diode
remarks ""
cycles 0.65625
progMem 0.18750
xmem 0.00000
ymem 0.00000
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "mode" 0..2 "0 ~ off, 1 ~ half wave, 2 ~ full wave"
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
83 Shaper
remarks ""
cycles 1.90625
progMem 0.46875
xmem 0.21875
ymem 0.09375
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "mode" 0..4 "0 ~ log2, 1 ~ log1, 2 ~ lin, 3 ~ exp1, 4 ~ exp2"
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
84 AD-Env
remarks ""
cycles 1.43750
progMem 0.87500
xmem 0.75000
ymem 0.21875
zeropage 1.75000
dynmem 0.37500
height 3
parameters
0 "attack" 0..127 "adsrtime"
1 "decay" 0..127 "adsrtime"
2 "gate" 0..1 "onoff"
inputs
0 "trigger" logic
1 "in" audio
2 "amp" control
outputs
0 "envelope" control
1 "out" audio
custom
----------
85 OscSlvFM
remarks ""
cycles 3.18750
progMem 0.71875
xmem 0.43750
ymem 0.28125
zeropage 0.87500
dynmem 0.50000
height 3
parameters
0 "detune coarse" 0..127 ""
1 "detune fine" 0..127 "symetric"
2 "-3oct" 0..1 "onoff"
3 "fm mod" 0..127 ""
4 "mute" 0..1 "onoff"
inputs
0 "mst" slave
1 "fm mod" audio
2 "sync" audio
outputs
0 "out" audio
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
86 FilterA
remarks ""
cycles 0.65625
progMem 0.18750
xmem 0.09375
ymem 0.09375
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "freq" 0..127 "filterfreqAB"
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
87 FilterB
remarks ""
cycles 1.03125
progMem 0.25000
xmem 0.09375
ymem 0.15625
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "freq" 0..127 "filterfreqAB"
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
88 1-4Switch
remarks ""
cycles 0.90625
progMem 0.21875
xmem 0.09375
ymem 0.00000
zeropage 3.50000
dynmem 0.37500
height 3
parameters
0 "sel" 0..3 "0 ~ out1, 3 ~ out4"
1 "level" 0..127 ""
2 "mute" 0..1 "onoff"
inputs
0 "in" audio
outputs
0 "out 1" audio
1 "out 2" audio
2 "out 3" audio
3 "out 4" audio
custom
----------
89 CompareAB
remarks ""
cycles 0.18750
progMem 0.18750
xmem 0.00000
ymem 0.00000
zeropage 0.87500
dynmem 0.25000
height 2
parameters
inputs
0 "A" control
1 "B" control
outputs
0 "A>=B" logic
custom
----------
90 NoteSeqB
remarks ""
cycles 1.43750
progMem 1.15625
xmem 0.56250
ymem 1.43750
zeropage 3.50000
dynmem 1.28125
height 9
parameters
0 "note 1" 0..127 "freqcoarse"
1 "note 2" 0..127 "freqcoarse"
2 "note 3" 0..127 "freqcoarse"
3 "note 4" 0..127 "freqcoarse"
4 "note 5" 0..127 "freqcoarse"
5 "note 6" 0..127 "freqcoarse"
6 "note 7" 0..127 "freqcoarse"
7 "note 8" 0..127 "freqcoarse"
8 "note 9" 0..127 "freqcoarse"
9 "note 10" 0..127 "freqcoarse"
10 "note 11" 0..127 "freqcoarse"
11 "note 12" 0..127 "freqcoarse"
12 "note 13" 0..127 "freqcoarse"
13 "note 14" 0..127 "freqcoarse"
14 "note 15" 0..127 "freqcoarse"
15 "note 16" 0..127 "freqcoarse"
16 "length" 0..15 ""
17 "currentstep" 0..16 "editpos"
18 "record" 0..1 "onoff"
19 "play" 0..1 "onoff"
20 "loop" 0..1 "onoff"
inputs
0 "clk" logic
1 "rst" logic
outputs
0 "out" control
1 "snc" logic
2 "link" logic
3 "gclk" logic
custom
0 "zoomfactor" 1..6 ""
1 "sliderposition" 6..117 ""
----------
91 CtrlSeq
remarks ""
cycles 1.43750
progMem 1.15625
xmem 0.56250
ymem 1.50000
zeropage 2.62500
dynmem 1.15625
height 7
parameters
0 "ctrl 1" 0..127 "unibi"
1 "ctrl 2" 0..127 "unibi"
2 "ctrl 3" 0..127 "unibi"
3 "ctrl 4" 0..127 "unibi"
4 "ctrl 5" 0..127 "unibi"
5 "ctrl 6" 0..127 "unibi"
6 "ctrl 7" 0..127 "unibi"
7 "ctrl 8" 0..127 "unibi"
8 "ctrl 9" 0..127 "unibi"
9 "ctrl 10" 0..127 "unibi"
10 "ctrl 11" 0..127 "unibi"
11 "ctrl 12" 0..127 "unibi"
12 "ctrl 13" 0..127 "unibi"
13 "ctrl 14" 0..127 "unibi"
14 "ctrl 15" 0..127 "unibi"
15 "ctrl 16" 0..127 "unibi"
16 "length" 0..15 ""
17 "uni" 0..1 "onoff"
18 "loop" 0..1 "onoff"
inputs
0 "clk" logic
1 "rst" logic
outputs
0 "out" control
1 "snc" logic
2 "link" logic
custom
----------
92 FilterF
remarks ""
cycles 5.53125
progMem 2.00000
xmem 0.68750
ymem 0.68750
zeropage 0.87500
dynmem 0.59375
height 6
parameters
0 "freq" 0..127 "filterfreq"
1 "kbt" 0..127 "freqkbt"
2 "res" 0..127 ""
3 "freq mod 1" 0..127 ""
4 "freq mod 2" 0..127 ""
5 "slope" 0..2 "filtertype1"
6 "bypass" 0..1 "onoff"
inputs
0 "freq mod 1" control
1 "freq mod 2" control
2 "in" audio
outputs
0 "out" audio
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
94 StereoChorus
remarks ""
cycles 9.12500
progMem 3.00000
xmem 18.09375
ymem 10.68750
zeropage 1.75000
dynmem 0.37500
height 3
parameters
0 "detune" 0..127 ""
1 "amount" 0..127 ""
2 "bypass" 0..1 "onoff"
inputs
0 "in" audio
outputs
0 "outleft" audio
1 "outright" audio
custom
----------
95 PercOsc
remarks ""
cycles 4.87500
progMem 1.53125
xmem 0.50000
ymem 0.50000
zeropage 0.87500
dynmem 0.59375
height 4
parameters
0 "freq coarse" 0..127 "0 ~ 8.18 Hz, 127 ~ 12.54 kHz"
1 "click" 0..127 ""
2 "decay" 0..127 ""
3 "punch" 0..1 "onoff"
4 "pitch mod" 0..127 ""
5 "freq fine" 0..127 "freqfine"
6 "mute" 0..1 "onoff"
inputs
0 "trig" audio
1 "am" audio
2 "pitch mod" control
outputs
0 "out" audio
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
96 FormantOsc
remarks ""
cycles 9.06250
progMem 2.53125
xmem 0.56250
ymem 0.50000
zeropage 1.75000
dynmem 0.59375
height 4
parameters
0 "freq coarse" 0..127 "freqcoarse"
1 "freq fine" 0..127 "freqfine"
2 "kbt" 0..1 "onoff"
3 "mute" 0..1 "onoff"
4 "timbre" 0..127 ""
5 "pitch mod 1" 0..127 ""
6 "pitch mod 2" 0..127 ""
inputs
0 "pitch mod 1" control
1 "pitch mod 2" control
2 "timbre" control
outputs
0 "out" audio
1 "slv" slave
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
97 MasterOsc
remarks ""
cycles 0.78125
progMem 0.68750
xmem 0.21875
ymem 0.15625
zeropage 0.87500
dynmem 0.50000
height 3
parameters
0 "freq coarse" 0..127 "freqcoarse"
1 "freq fine" 0..127 "freqfine"
2 "kbt" 0..1 "onoff"
3 "pitch mod 1" 0..127 ""
4 "pitch mod 2" 0..127 ""
inputs
0 "pitch mod 1" control
1 "pitch mod 2" control
outputs
0 "slv" slave
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
98 KeyQuant
remarks ""
cycles 1.34375
progMem 1.18750
xmem 1.03125
ymem 1.03125
zeropage 0.87500
dynmem 0.90625
height 4
parameters
0 "range" 0..127 "symetric"
1 "cont" 0..1 "onoff"
2 "E" 0..1 "onoff"
3 "F" 0..1 "onoff"
4 "F#" 0..1 "onoff"
5 "G" 0..1 "onoff"
6 "G#" 0..1 "onoff"
7 "A" 0..1 "onoff"
8 "A#" 0..1 "onoff"
9 "B" 0..1 "onoff"
10 "C" 0..1 "onoff"
11 "C#" 0..1 "onoff"
12 "D" 0..1 "onoff"
13 "D#" 0..1 "onoff"
inputs
0 "in" control
outputs
0 "out" control
custom
----------
99 PatternGen
remarks ""
cycles 2.34375
progMem 1.53125
xmem 0.50000
ymem 0.34375
zeropage 0.87500
dynmem 0.46875
height 4
parameters
0 "pattern" 0..127 ""
1 "bank" 0..127 ""
2 "low delta" 0..1 "onoff"
3 "step" 0..127 ""
4 "mono" 0..1 "onoff"
inputs
0 "clk" logic
1 "rst" logic
2 "pattern & bank" control
outputs
0 "out" control
custom
----------
100 KeyboardSplit
remarks "only 1"
cycles 0.79000
progMem 1.00000
xmem 1.00000
ymem 1.00000
zeropage 3.00000
dynmem 1.00000
height 3
parameters
0 "upper" 0..127 "freqcoarse"
1 "lower" 0..127 "freqcoarse"
inputs
0 "note" control
1 "gate" logic
2 "vel" control
outputs
0 "note" control
1 "gate" logic
2 "vel" control
custom
----------
102 Phaser
remarks ""
cycles 12.56250
progMem 3.40625
xmem 1.15625
ymem 1.09375
zeropage 0.87500
dynmem 0.78125
height 7
parameters
0 "rate" 0..127 "0 ~ 62.9 s, 127 ~ 24.4 hHz"
1 "lfo" 0..1 "onoff"
2 "freq mod" 0..127 ""
3 "freq" 0..127 "0 ~ 100 Hz, 127 ~ 16 kHz"
4 "spread mod" 0..127 ""
5 "feedback" 0..127 ""
6 "peaks" 0..5 "0 ~ 1 peak, 5 ~ 6 peaks"
7 "spread" 0..127 ""
8 "bypass" 0..1 "onoff"
9 "depth" 0..127 ""
10 "level" 0..127 ""
inputs
0 "in" audio
1 "freq mod" control
2 "spread mod" control
outputs
0 "out" audio
custom
----------
103 EqMid
remarks ""
cycles 3.34375
progMem 1.06250
xmem 0.34375
ymem 0.56250
zeropage 0.87500
dynmem 0.46875
height 4
parameters
0 "freq" 0..127 "eqfreq"
1 "gain" 0..127 "eqgain"
2 "bandwidth" 0..127 "0 ~ 2 oct, 64 ~ 1 oct, 127 ~ 0.02 oct"
3 "bypass" 0..1 "onoff"
4 "level" 0..127 ""
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
104 EqShelving
remarks ""
cycles 2.43750
progMem 0.56250
xmem 0.21875
ymem 0.15625
zeropage 0.87500
dynmem 0.46875
height 4
parameters
0 "freq" 0..127 "eqfreq"
1 "gain" 0..127 "eqgain"
2 "mode" 0..1 "0 ~ low, 1 ~ high"
3 "bypass" 0..1 "onoff"
4 "level" 0..127 ""
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
105 Expander
remarks ""
cycles 8.28125
progMem 1.81250
xmem 0.68750
ymem 0.62500
zeropage 1.75000
dynmem 0.68750
height 7
parameters
0 "attack" 0..127 "companderattack"
1 "release" 0..127 "companderrelease"
2 "treshold" 0..84 "compandertreshold"
3 "ratio" 0..66 "companderratio"
4 "gate" 0..72 "compandergate"
5 "hold" 0..127 "companderhold"
6 "act" 0..1 "onoff"
7 "mon" 0..1 "onoff"
8 "bypass" 0..1 "onoff"
inputs
0 "in left" audio
1 "in right" audio
2 "sidechain" audio
outputs
0 "out left" audio
1 "out right" audio
custom
----------
106 OscSineBank
remarks ""
cycles 16.78125
progMem 3.56250
xmem 0.84375
ymem 2.25000
zeropage 0.87500
dynmem 1.40625
height 10
parameters
0 "osc1 coarse" 0..127 ""
1 "osc1 fine" 0..127 "symetric"
2 "osc1 level" 0..127 ""
3 "osc2 coarse" 0..127 ""
4 "osc2 fine" 0..127 "symetric"
5 "osc2 level" 0..127 ""
6 "osc3 coarse" 0..127 ""
7 "osc3 fine" 0..127 "symetric"
8 "osc3 level" 0..127 ""
9 "osc4 coarse" 0..127 ""
10 "osc4 fine" 0..127 "symetric"
11 "osc4 level" 0..127 ""
12 "osc5 coarse" 0..127 ""
13 "osc5 fine" 0..127 "symetric"
14 "osc5 level" 0..127 ""
15 "osc6 coarse" 0..127 ""
16 "osc6 fine" 0..127 "symetric"
17 "osc6 level" 0..127 ""
18 "osc1 mute" 0..1 "onoff"
19 "osc2 mute" 0..1 "onoff"
20 "osc3 mute" 0..1 "onoff"
21 "osc4 mute" 0..1 "onoff"
22 "osc5 mute" 0..1 "onoff"
23 "osc6 mute" 0..1 "onoff"
inputs
0 "mst" slave
1 "mixin" audio
2 "sync" audio
3 "osc1 am" audio
4 "osc2 am" audio
5 "osc3 am" audio
6 "osc4 am" audio
7 "osc5 am" audio
8 "osc6 am" audio
outputs
0 "out" audio
custom
----------
107 SpectralOsc
remarks ""
cycles 7.90625
progMem 2.40625
xmem 0.50000
ymem 0.75000
zeropage 1.75000
dynmem 0.75000
height 5
parameters
0 "freq coarse" 0..127 "freqcoarse"
1 "freq fine" 0..127 "freqfine"
2 "shape" 0..127 ""
3 "partials" 0..1 "0 ~ odd, 1 ~ all"
4 "pitch mod 1" 0..127 ""
5 "pitch mod 2" 0..127 ""
6 "fm mod" 0..127 ""
7 "shape mod" 0..127 ""
8 "kbt" 0..1 "onoff"
9 "mute" 0..1 "onoff"
inputs
0 "fm mod" audio
1 "pitch mod 1" control
2 "pitch mod 2" control
3 "shape mod" control
outputs
0 "out" audio
1 "slv" slave
custom
0 "freq display units" 0..1 "freqdisplunits"
----------
108 Vocoder
remarks ""
cycles 48.93750
progMem 34.21875
xmem 23.78125
ymem 26.71875
zeropage 0.87500
dynmem 15.00000
height 8
parameters
0 "band 1" 0..16 "vocoband"
1 "band 2" 0..16 "vocoband"
2 "band 3" 0..16 "vocoband"
3 "band 4" 0..16 "vocoband"
4 "band 5" 0..16 "vocoband"
5 "band 6" 0..16 "vocoband"
6 "band 7" 0..16 "vocoband"
7 "band 8" 0..16 "vocoband"
8 "band 9" 0..16 "vocoband"
9 "band 10" 0..16 "vocoband"
10 "band 11" 0..16 "vocoband"
11 "band 12" 0..16 "vocoband"
12 "band 13" 0..16 "vocoband"
13 "band 14" 0..16 "vocoband"
14 "band 15" 0..16 "vocoband"
15 "band 16" 0..16 "vocoband"
16 "outgain" 0..127 ""
17 "emphasis" 0..1 ""
18 "monitor" 0..1 ""
inputs
0 "control" audio
1 "in" audio
outputs
0 "out" audio
custom
----------
110 RandomGen
remarks ""
cycles 1.43750
progMem 1.18750
xmem 0.50000
ymem 0.34375
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "rate" 0..127 "lfoslvrate"
inputs
0 "mst" slave
outputs
0 "out" control
custom
----------
111 LevMult
remarks ""
cycles 0.53125
progMem 0.15625
xmem 0.09375
ymem 0.00000
zeropage 0.87500
dynmem 0.34375
height 2
parameters
0 "gain" 0..127 "unibi"
1 "unipolar" 0..1 ""
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
112 LevAdd
remarks ""
cycles 0.53125
progMem 0.15625
xmem 0.09375
ymem 0.00000
zeropage 0.87500
dynmem 0.34375
height 2
parameters
0 "level" 0..127 "unibi"
1 "unipolar" 0..1 ""
inputs
0 "in" audio
outputs
0 "out" audio
custom
----------
113 1to2Fade
remarks ""
cycles 0.78125
progMem 0.21875
xmem 0.09375
ymem 0.09375
zeropage 1.75000
dynmem 0.28125
height 2
parameters
0 "mix" 0..127 "symetric"
inputs
0 "in" audio
outputs
0 "out 1" audio
1 "out 2" audio
custom
----------
114 2to1Fade
remarks ""
cycles 0.78125
progMem 0.21875
xmem 0.09375
ymem 0.00000
zeropage 0.87500
dynmem 0.28125
height 2
parameters
0 "mix" 0..127 "symetric"
inputs
0 "in 1" audio
1 "in 2" audio
outputs
0 "out" audio
custom
----------
115 NoteVelScal
remarks ""
cycles 0.87500
progMem 0.78125
xmem 0.34375
ymem 0.34375
zeropage 0.87500
dynmem 0.43750
height 4
parameters
0 "velocity sensitivity" 0..127 ""
1 "left gain" 0..48 "velscalgain"
2 "breakpoint" 0..127 "freqcoarse"
3 "right gain" 0..48 "velscalgain"
inputs
0 "velocity" control
1 "note" control
outputs
0 "out" control
custom
----------
117 RingMod
remarks ""
cycles 1.90625
progMem 0.43750
xmem 0.09375
ymem 0.15625
zeropage 0.87500
dynmem 0.34375
height 3
parameters
0 "mod depth" 0..127 ""
1 "ringmod depth" 0..127 "0 ~ 0, 64 ~ AM, 127 ~ RM"
inputs
0 "in" audio
1 "mod" audio
2 "mod depth" audio
outputs
0 "out" audio
custom
----------
118 Digitizer
remarks ""
cycles 3.43750
progMem 0.78125
xmem 0.28125
ymem 0.21875
zeropage 0.43750
dynmem 0.46875
height 3
parameters
0 "bits" 0..11 "quantbits"
1 "rate" 0..127 "0 ~ 34.65 Hz, 127 ~ 50.18 kHz"
2 "rate mod" 0..127 ""
3 "quant off" 0..1 "onoff"
4 "sampling off" 0..1 "onoff"
inputs
0 "in" audio
1 "rate mod" control
outputs
0 "out" audio
custom
----------
127 PolyAreaIn
remarks "only 1"
cycles 2.20000
progMem 1.00000
xmem 1.00000
ymem 1.00000
zeropage 2.00000
dynmem 1.00000
height 2
parameters
0 "+6db" 0..1 "onoff"
inputs
outputs
0 "Left" audio
1 "Right" audio
custom
----------
